IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-09-03T15:58:00"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.0.0.420 - Default UI"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "bpfluid" of Organization (no name given)
  Owner history of Person "bpfluid" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1567519075 (2019-09-03T13:57:55Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350" | object type "GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350" | names: "GRYFIT CX-5, Fire damper:GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350:916629" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, General, Identity Data, Insulation

Types
  IFCBUILDINGELEMENTPROXYTYPE "GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350" | 1 occurrence | property sets: Dimensions, General, Identity Data, Other

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.110066577640957 (IFCAREAMEASURE) [SQUARE_METRE]
    Damper Height = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Damper Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "100ø-100ø" (IFCTEXT)
    Symbol Width = 450. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00353585349686065 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Damper Length = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    anglXY1 = 180. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    anglXY2 = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    anglZ1 = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    anglZ2 = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    diamcon1 = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    diamcon2 = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    lengX1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    lengX2 = 175. (IFCLENGTHMEASURE) [MILLI METRE]
    lengXY1 = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    lengXY2 = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    lengXYZ1 = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    lengXYZ2 = 542.5 (IFCLENGTHMEASURE) [MILLI METRE]
    lengY1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    lengY2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    lengZ1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    lengZ2 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    instID = "D100.FDINS0001" (IFCTEXT)
  General | properties | on 1 type object
    95°C = "" (IFCTEXT)
    Access door = FALSE (IFCBOOLEAN)
    Actuator type. = "FDG-WT-8" (IFCTEXT)
    Actuator voltage. = "24/48 V AC/DC" (IFCTEXT)
    Application in mixed systems (SM) = FALSE (IFCBOOLEAN)
    Assembly in light wall = FALSE (IFCBOOLEAN)
    Communication and power supply unit. = "" (IFCTEXT)
    Compact index = FALSE (IFCBOOLEAN)
    Damper casing tightness class. = "C (EN 1751:2002)" (IFCTEXT)
    Damper tightness class. = "4 (EN 1751:2002)" (IFCTEXT)
    Diameter (D). = "100" (IFCTEXT)
    Double Beginning and End (2WKKP) = "None" (IFCTEXT)
    EMS module = TRUE (IFCBOOLEAN)
    EPDM Gaskets = FALSE (IFCBOOLEAN)
    Electromagnet = FALSE (IFCBOOLEAN)
    Electromagnet type. = "" (IFCTEXT)
    Electromagnet voltage. = "" (IFCTEXT)
    Fire resistance class. = "EI 120(ve-ho-i<->o)S (EN 13501-3+A1:2010)" (IFCTEXT)
    Geometry = "GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350" (IFCLABEL)
    Installation Brackets = TRUE (IFCBOOLEAN)
    Installation opening diam. (Dr). = "150" (IFCTEXT)
    Length (P). = "350" (IFCTEXT)
    Material. = "Galvanized steel" (IFCTEXT)
    Mechanism cover = FALSE (IFCBOOLEAN)
    Thickness of wall (G). = "115" (IFCTEXT)
    Type. = "GRYFIT CX-5" (IFCTEXT)
    Without function separation (BRF) = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "23.75.70.11.14.14" (IFCTEXT)
    OmniClass Title = "Dampers for Air Ductwork" (IFCTEXT)
    Type Name = "GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350" (IFCTEXT)
  Insulation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "100 mmø-100 mmø" (IFCTEXT)
  Lining | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Free Size = "100 mmø-100 mmø" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Loss Method = "8baf7d75-8b9b-46d0-b8ce-3ad1c19e6b19" (IFCTEXT)
    Pressure Drop = 249. (IFCPRESSUREMEASURE) [PASCAL]
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Duct Accessories" (IFCLABEL)
    Family = "GRYFIT CX-5, Fire damper: GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350" (IFCLABEL)
    Family and Type = "GRYFIT CX-5, Fire damper: GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350" (IFCLABEL)
    Half Damper Height = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Half Damper Width = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Half Symbol Width = 225. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "GRYFIT CX-5, Fire damper: GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350" (IFCLABEL)
    Type Id = "GRYFIT CX-5, Fire damper: GRYFIT CX-5, D=100, Galvanized steel, EMS + FDG-WT-8-24 + UM, D=100. P=350" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Duct Accessories" (IFCLABEL)
    Family Name = "GRYFIT CX-5, Fire damper" (IFCTEXT)
    Half Damper Length = 75. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)