IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2020-02-24T21:19:38"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Default UI"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "olegog" of Organization (no name given)
  Owner history of Person "olegog" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 1582571977 (2020-02-24T19:19:37Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750" | object type "GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750" | names: "GRYFIT NEO, Multiblade fire damper:GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750:918426" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, General, Identity Data, Insulation

Types
  IFCBUILDINGELEMENTPROXYTYPE "GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750" | 1 occurrence | property sets: Dimensions, General, Identity Data, Other

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 1.415069 (IFCAREAMEASURE) [SQUARE_METRE]
    Damper Height = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Damper Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "700x750" (IFCTEXT)
    Symbol Width = 450. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0763411800000001 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Damper Length = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    anglXY1 = 180. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    anglZ1 = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    heightcon1 = 750. (IFCLENGTHMEASURE) [MILLI METRE]
    lengX1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    lengXY1 = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    lengXYZ1 = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    lengY1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    lengZ1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    rotcon1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    widthcon1 = 700. (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    instID = "L700xH750.FDINS0001" (IFCTEXT)
  General | properties | on 1 type object
    95°C = "" (IFCTEXT)
    Actuator FDG-8 = FALSE (IFCBOOLEAN)
    Actuator FDG-WT-5 = FALSE (IFCBOOLEAN)
    Actuator FDG-WT-8 = FALSE (IFCBOOLEAN)
    Actuator voltage. = "" (IFCTEXT)
    Colour of grill. = "" (IFCTEXT)
    Connector. = "Rectangular flange 30 mm" (IFCTEXT)
    Damper external hight (H1). = "813" (IFCTEXT)
    Damper external width (L1). = "763" (IFCTEXT)
    Dimensions as 5 mm in the standard. = FALSE (IFCBOOLEAN)
    Double Beginning and End (2WKKP) = "None" (IFCTEXT)
    EMS module = FALSE (IFCBOOLEAN)
    Electromagnet = FALSE (IFCBOOLEAN)
    Electromagnet type. = "" (IFCTEXT)
    Electromagnet voltage. = "" (IFCTEXT)
    Fire resistance class. = "EIS 120" (IFCTEXT)
    Gap between grille and damper (G1). = "0" (IFCTEXT)
    Geometry = "GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750" (IFCLABEL)
    Grille external height (Hg). = "870" (IFCTEXT)
    Grille external width (Lg). = "820" (IFCTEXT)
    Height (H). = "750" (IFCTEXT)
    Height (Hk). = "750" (IFCTEXT)
    Height of mount. hole (Hr). = "850" (IFCTEXT)
    Length (P). = "120" (IFCTEXT)
    Material of damper. = "Galvanized steel" (IFCTEXT)
    Material of grille. = "" (IFCTEXT)
    Protection grille (TRA) = FALSE (IFCBOOLEAN)
    Type. = "GRYFIT NEO" (IFCTEXT)
    Width (L). = "700" (IFCTEXT)
    Width (Lk). = "700" (IFCTEXT)
    Width as 5mm (L 5mm). = "100" (IFCTEXT)
    Width of mount. hole (Lr). = "800" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "23.75.70.11.14.14" (IFCTEXT)
    OmniClass Title = "Dampers for Air Ductwork" (IFCTEXT)
    Type Name = "GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750" (IFCTEXT)
  Insulation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "700 mmx750 mm" (IFCTEXT)
  Lining | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Free Size = "700 mmx750 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Loss Method = "8baf7d75-8b9b-46d0-b8ce-3ad1c19e6b19" (IFCTEXT)
    Pressure Drop = 249. (IFCPRESSUREMEASURE) [PASCAL]
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Duct Accessories" (IFCLABEL)
    Family = "GRYFIT NEO, Multiblade fire damper: GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750" (IFCLABEL)
    Family and Type = "GRYFIT NEO, Multiblade fire damper: GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750" (IFCLABEL)
    Half Damper Height = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Half Damper Width = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Half Symbol Width = 225. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "GRYFIT NEO, Multiblade fire damper: GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750" (IFCLABEL)
    Type Id = "GRYFIT NEO, Multiblade fire damper: GRYFIT NEO, LxH=700x750,Galvanized steel, KP 30 + , TRA, L=700. H=750" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Duct Accessories" (IFCLABEL)
    Family Name = "GRYFIT NEO, Multiblade fire damper" (IFCTEXT)
    Half Damper Length = 75. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)