IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-06-01T14:06:08"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.0.0.420 - Default UI"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "bpfluid" of Organization (no name given)
  Owner history of Person "bpfluid" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1559390765 (2019-06-01T12:06:05Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCAIRTERMINALTYPE "GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150" | object type "GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150" | names: "GRYFIT BX-1H, Fire valve:GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150:916982" | property sets: Pset_DistributionFlowElementCommon, Constraints, Dimensions, General, Identity Data, Mechanical

Types
  IFCAIRTERMINALTYPE "GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150" | 1 occurrence | property sets: Dimensions, General, Identity Data, Other

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWTERMINAL)
    Reference = "GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.0977570034239799 (IFCAREAMEASURE) [SQUARE_METRE]
    Size = "200ø" (IFCTEXT)
    Volume = 0.00397196429373372 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Diffuser Height = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Diffuser Width = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Duct Height = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Duct Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    anglXY1 = 180. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    anglZ1 = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    diamcon1 = 200. (IFCLENGTHMEASURE) [MILLI METRE]
    lengX1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    lengXY1 = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    lengXYZ1 = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    lengY1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    lengZ1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCFLOWTERMINAL)
    instID = "D200_KM67.FDINS0001" (IFCTEXT)
  General | properties | on 1 type object
    72°C = "72°C" (IFCTEXT)
    Beginning and End (1WKKP) = "None" (IFCTEXT)
    Body collar width (H). = "20" (IFCTEXT)
    Diameter (D). = "200" (IFCTEXT)
    Diameter of body (DK). = "252" (IFCTEXT)
    Diameter of mounting hole (Dr). = "240" (IFCTEXT)
    Electromagnet = FALSE (IFCBOOLEAN)
    Electromagnet type. = "" (IFCTEXT)
    Electromagnet voltage. = "" (IFCTEXT)
    Fire resistance class. = "EIS 60" (IFCTEXT)
    Geometry = "GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150" (IFCLABEL)
    Length of valve (P). = "150" (IFCTEXT)
    Mounting collar (KM). = "67" (IFCTEXT)
    Type. = "GRYFIT BX-1H" (IFCTEXT)
    Value (B). = "93" (IFCTEXT)
    Width of gap (S). = "6" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "23.75.70.21.27.11" (IFCTEXT)
    OmniClass Title = "Diffusers, Registers, and Grilles" (IFCTEXT)
    Type Name = "GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWTERMINAL)
    DownArrow = TRUE (IFCBOOLEAN)
    LeftArrow = TRUE (IFCBOOLEAN)
    RightArrow = TRUE (IFCBOOLEAN)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "" (IFCTEXT)
    UpArrow = TRUE (IFCBOOLEAN)
  Mechanical - Flow | properties | on 1 object (1 IFCFLOWTERMINAL)
    Flow = 8.29894667954982 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Pressure Drop = 14. (IFCPRESSUREMEASURE) [PASCAL]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    Category = "Air Terminals" (IFCLABEL)
    Family = "GRYFIT BX-1H, Fire valve: GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150" (IFCLABEL)
    Family and Type = "GRYFIT BX-1H, Fire valve: GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150" (IFCLABEL)
    Type = "GRYFIT BX-1H, Fire valve: GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150" (IFCLABEL)
    Type Id = "GRYFIT BX-1H, Fire valve: GRYFIT BX-1H, D=200 + KM, KM=67 + WT72C, D=200. DK=252. S=6. P=150" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Air Terminals" (IFCLABEL)
    Family Name = "GRYFIT BX-1H, Fire valve" (IFCTEXT)
    Width 1 = 390. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 1 object (1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)