IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2020-02-22T13:44:20"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190808_0900(x64) - Exporter 19.2.20.24 - Default UI"
Application: "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)"

People and organizations
  Person "olegog" of Organization (no name given)
  Owner history of Person "olegog" of Organization (no name given) | application "Autodesk Revit 2019 (ENU)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENU)" | change NOCHANGE | created 1582371859 (2020-02-22T11:44:19Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 12′ 46.799999″ | longitude -71° 1′ 58.799999″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668" | object type "GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668" | names: "GRYFIT VX-6V, Smoke damper:GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668:918428" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, General, Identity Data, Insulation

Types
  IFCBUILDINGELEMENTPROXYTYPE "GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668" | 1 occurrence | property sets: Dimensions, General, Identity Data, Other

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 1.5645549 (IFCAREAMEASURE) [SQUARE_METRE]
    Damper Height = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Damper Width = 300. (IFCLENGTHMEASURE) [MILLI METRE]
    Size = "637x668" (IFCTEXT)
    Symbol Width = 450. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.033301207 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Damper Length = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    anglXY1 = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    anglZ1 = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    heightcon1 = 668. (IFCLENGTHMEASURE) [MILLI METRE]
    lengX1 = 57.5 (IFCLENGTHMEASURE) [MILLI METRE]
    lengXY1 = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    lengXYZ1 = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    lengY1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    lengZ1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    rotcon1 = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    widthcon1 = 637. (IFCLENGTHMEASURE) [MILLI METRE]
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    instID = "L637xH668.FDINS0001" (IFCTEXT)
  General | properties | on 1 type object
    Actuator type. = "None" (IFCTEXT)
    Actuator voltage. = "" (IFCTEXT)
    Colour of ext. grille. = "natural" (IFCTEXT)
    Damper mounting frame (RM) = TRUE (IFCBOOLEAN)
    Damper opening direction. = "right/left" (IFCTEXT)
    Double Beginning and End (2WKKP) = "Beginning and End (1WKKP)" (IFCTEXT)
    Electromagnet = TRUE (IFCBOOLEAN)
    Electromagnet type. = "impulse" (IFCTEXT)
    Electromagnet voltage. = "24/48 V DC" (IFCTEXT)
    External grille assembly. = "hinges" (IFCTEXT)
    External louvre. = "GHPV" (IFCTEXT)
    Fire resistance class. = "EI 120 (ved i↔o) S 1500Pa AA multi" (IFCTEXT)
    Geometry = "GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668" (IFCLABEL)
    Height (H). = "668" (IFCTEXT)
    Height (Hge). = "742" (IFCTEXT)
    Height (Hht). = "697" (IFCTEXT)
    Height (Hl). = "604" (IFCTEXT)
    Height (Hr). = "688" (IFCTEXT)
    Length (P). = "438.5" (IFCTEXT)
    Material of ext. grille. = "Aluminium" (IFCTEXT)
    Material. = "Galvanized steel" (IFCTEXT)
    Protection grille. = TRUE (IFCBOOLEAN)
    Type. = "VX-6-V, EI120S, 2V" (IFCTEXT)
    Width (L). = "637" (IFCTEXT)
    Width (Lge). = "713" (IFCTEXT)
    Width (Lht). = "685" (IFCTEXT)
    Width (Ll). = "594" (IFCTEXT)
    Width (Lr). = "657" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "23.75.70.11.14.14" (IFCTEXT)
    OmniClass Title = "Dampers for Air Ductwork" (IFCTEXT)
    Type Name = "GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668" (IFCTEXT)
  Insulation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Insulation Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Size = "637 mmx668 mm" (IFCTEXT)
  Lining | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Free Size = "637 mmx668 mm" (IFCTEXT)
    Lining Thickness = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Loss Method = "8baf7d75-8b9b-46d0-b8ce-3ad1c19e6b19" (IFCTEXT)
    Pressure Drop = 249. (IFCPRESSUREMEASURE) [PASCAL]
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Supply Air" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Duct Accessories" (IFCLABEL)
    Family = "GRYFIT VX-6V, Smoke damper: GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668" (IFCLABEL)
    Family and Type = "GRYFIT VX-6V, Smoke damper: GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668" (IFCLABEL)
    Half Damper Height = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Half Damper Width = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Half Symbol Width = 225. (IFCLENGTHMEASURE) [MILLI METRE]
    Type = "GRYFIT VX-6V, Smoke damper: GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668" (IFCLABEL)
    Type Id = "GRYFIT VX-6V, Smoke damper: GRYFIT VX-6V (2H,2V), LxH=637x668 + EI24 + 1WKKP + GHPV + RM, LxH=637x668" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Duct Accessories" (IFCLABEL)
    Family Name = "GRYFIT VX-6V, Smoke damper" (IFCTEXT)
    Half Damper Length = 75. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)